MIT GNU Public License 

X = 2048, Y = 512 

6 iterations, with angle 40 deg

laf_nashr*.caf

{
image= lsys_laff _nashr2.jpg
rules={{"f" -> "f[+f]ff[-f]"}, "f"}

x-axis reflection and y-reflection 

MAP=micro 50
REVERB=64 (Grid)
MultiSampler = All AEIO Cycle (VOICES) 
A2 or A1...
Stereo
reverb16
BPM=20
}